Remark：

1. The inspection interval is *Monthly*；
2. Mainly to check batteries’ electrolyte level, cell voltage(2.23 V/cell ± 1 %) and electrolyte density(Rated value is 1.24mg/ml)；
3. Make a good inspection record. If any abnormality is found, please inform the responsible person of the situation in time and take corresponding measures with the permission of the responsible person。

备注：

1. 蓄电池每月巡检一次；
2. 主要检查蓄电池的液面高度，蓄电池单体电压（2.23 V/cell ± 1 %）和电解质密度（额定值1.24mg/ml）
3. 做好巡检记录，如发现异常请及时向负责人说明情况，并在负责人许可的情况下采取相应的措施。